FR-AG-005 — Deployment Traceability Across Disconnected Environments

Go to Crucible Air-Gapped Operations Requirements

Statement

Crucible SHALL maintain Deployment Traceability across Disconnected Environments.

Derived From

This requirement derives from:

Crucible System Requirements Specification, Version 1.1 Draft, Functional Requirements, FR-AG-005The Original Requirement states:

The system shall maintain deployment traceability across disconnected environments.[C1]

FR-AG-005:

Replaces The system with the defined system name CrucibleChanges shall to the established uppercase normative form SHALLLinks Deployment, Traceability, and Disconnected Environments to their controlling definitionsNo other substantive normalization is required.

Rationale

Deployment Traceability allows an evaluator to relate a deployment performed within a Disconnected Environment to the controlled information associated with that deployment.

Relevant traceability information can include relationships among:

Deployment inputsDeployment operationsDeployment resultsBaselinesArtifactsTransfer recordsValidation resultsEvidenceThis requirement does not prescribe:

A particular set of traceability relationshipsA centralized traceability repositoryDirect network communication among Disconnected EnvironmentsA traceability data modelAn identifier formatA transfer mechanismA repository implementationSeparate requirements, architecture specifications, workflows, or policies define those subjects.

Applies To

This requirement applies to:

Verification

Verification confirms that:

A Deployment involving one or more Disconnected Environments is selected for testingTraceability information associated with the tested Deployment is identifiedCrucible maintains the identified Deployment Traceability across the tested Disconnected EnvironmentsThe maintained traceability information allows the tested Deployment and its associated controlled information to be relatedThe traceability information remains available without requiring prohibited direct communication between the tested Disconnected Environments

Referenced By

The following pages reference this requirement:

Implementation Status

Implemented and Verified

Requirement Status

Issues

Notes for Editors

This requirement page retains the stable requirement identifier FR-AG-005.

This page is a leaf requirement page and omits a trailing :start from its namespace.

The Statement preserves the approved source intent by requiring Crucible to maintain Deployment Traceability across Disconnected Environments.

Do not add a mandatory list of source Baselines, transferred Artifacts, deployment inputs, deployment results, transfer records, or Evidence to the Statement unless the controlling requirement changes through an approved requirements process.

Do not interpret across Disconnected Environments as requiring direct network communication between those environments.

To reference this requirement Statement from another wiki page, insert:

{{section>dido:02-crusible:99-annexes:annex-c-requirements:03-functional-requirements:03-05-air-gap-operations:fr-ag-005#Statement&noheader&nofooter&noeditbtn}}

© 2026 Dido Solutions, Inc. and Jackrabbit Consulting, Inc.