ENV-002e — Apply Configuration Values

Go to ENV-002 — Configure Test Environment

Statement

The DIDO-TE SHALL apply each specified Configuration value to the applicable element of a Test Environment before Test Execution.

Derived From

, source requirement identifier and obligation to be assigned[DTE6] Structured Information Processing Reference Architecture (SIP-RA)[DTE7] Federated Data Interpretation Systems Reference Architecture (FDIS-RA)

Rationale

Applying each specified Configuration value establishes the required operating state of every configurable element within a Test Environment.

The applied values govern the behaviour of Test Objects, Nodes, Test Resources, communication mechanisms, and supporting services during Test Execution.

Recording and verifying the applied values supports controlled execution, Reproducibility, and assessment of whether a Configuration difference influenced a Test Result.

Applies To

Verification

Verification confirms that:

The DIDO-TE identifies every Configuration value specified for the Test Environment.The DIDO-TE applies each specified Configuration value to its applicable Test Environment element.Each applied Configuration value has the specified name, value, data type, unit, format, and scope, when applicable.Each configured element exposes or otherwise provides evidence of its applied Configuration values.The DIDO-TE records the applied Configuration values as part of the resulting Test Environment Configuration.The DIDO-TE maintains Traceability between each specified Configuration value and its applied value.A missing, incorrect, invalid, or untraceable Configuration value constitutes nonconformance with this requirement.Verification includes:

Inspection of the Configuration values specified for the Test EnvironmentInspection of the Configuration values applied to each applicable Test Environment elementComparison of each applied Configuration value with its controlled specificationInspection of the resulting Test Environment ConfigurationInspection of Traceability records connecting each specified Configuration value to its applied valueA negative assessment using a missing, incorrect, invalid, or untraceable Configuration valueConfirmation that the negative assessment produces a nonconformance result

Referenced By

Related Architecture Sections

Add links to the architecture sections governing Test Environment Configuration, Configuration values, configuration control, and validation.

Delivery Phase

Assign the applicable delivery phase.

Requirement Status

Draft

Statement Reference

Use the following syntax to reference this requirement’s Statement section from another DokuWiki page:

{{section>dido:03-dido-te:99-annexes:annex-c-requirements:02-test-environment-requirements:env-002-configure-test-environment:env-002e-apply-configuration-values#Statement&noheader&nofooter&noeditbtn}}

© 2026 Dido Solutions, Inc. and Jackrabbit Consulting, Inc.