ENV-003e — Provision Required Test Resources

Go to ENV-003 — Establish Controlled Starting State

Statement

Before each Test Execution, the DIDO-TE SHALL provision each Test Resource specified by the controlled descriptive information governing the applicable Test Environment.

Derived From

, source requirement identifier and obligation to be assigned[DTE6] Structured Information Processing Reference Architecture (SIP-RA)[DTE7] Federated Data Interpretation Systems Reference Architecture (FDIS-RA)

Rationale

Provisioning the required Test Resources supplies the infrastructure, services, software, data, devices, credentials, storage, network capacity, and supporting capabilities required by a Test Execution.

Each provisioned Test Resource must correspond to the type, quantity, capacity, version, location, and Configuration specified by the controlled descriptive information.

Controlled provisioning prevents missing, unsuitable, incorrectly configured, or unapproved resources from affecting Test Execution or the interpretation of the resulting Test Results.

Applies To

Verification

Verification confirms that:

The controlled descriptive information identifies each Test Resource required for the Test Execution.The controlled descriptive information specifies the required type, quantity, capacity, version, location, Configuration, and availability of each Test Resource.The DIDO-TE provisions each required Test Resource before Test Execution.Each provisioned Test Resource corresponds to its specified characteristics.Each provisioned Test Resource is available to the applicable Node, Test Object, or Test Procedure.The provisioned Test Resources exclude unapproved, obsolete, conflicting, and prohibited resources.The DIDO-TE records the identity, version, Configuration, location, provisioning status, and availability of each Test Resource.The DIDO-TE maintains Traceability among each required Test Resource, its specification, its consumer, the Test Environment, and the applicable Test Execution.A missing, unavailable, unsuitable, incorrectly configured, unapproved, obsolete, or untraceable Test Resource constitutes nonconformance with this requirement.Verification includes:

Inspection of the controlled descriptive information identifying each required Test ResourceInspection of the specified characteristics of each Test ResourceObservation of Test Resource provisioningComparison of each provisioned Test Resource with its specified type, quantity, capacity, version, location, and ConfigurationConfirmation of Test Resource availability to the applicable Node, Test Object, or Test ProcedureInspection for unapproved, obsolete, conflicting, and prohibited Test ResourcesInspection of Test Resource identity, version, Configuration, location, provisioning-status, and availability recordsInspection of Traceability records connecting each Test Resource to its specification, consumer, Test Environment, and Test ExecutionA negative assessment using a missing, unavailable, unsuitable, incorrectly configured, unapproved, obsolete, or untraceable Test ResourceConfirmation that the negative assessment produces a nonconformance result

Referenced By

Related Architecture Sections

Add links to the architecture sections governing Test Resource specification, provisioning, Configuration, availability, Deployment Targets, and Test Execution admission.

Delivery Phase

Assign the applicable delivery phase.

Requirement Status

Draft

Statement Reference

Use the following syntax to reference this requirement’s Statement section from another DokuWiki page:

{{section>dido:03-dido-te:99-annexes:annex-c-requirements:02-test-environment-requirements:env-003-establish-controlled-starting-state:env-003e-provision-required-test-resources#Statement&noheader&nofooter&noeditbtn}}

© 2026 Dido Solutions, Inc. and Jackrabbit Consulting, Inc.