NOD-003d — Establish Node Bindings

Go to NOD-003 — Configure a Node

Statement

The DIDO-TE SHALL establish each Node Binding required by a configured Node.

Derived From

, source requirement identifier and obligation to be assigned[DTE6] Structured Information Processing Reference Architecture (SIP-RA)[DTE7] Federated Data Interpretation Systems Reference Architecture (FDIS-RA)

Rationale

A Node Binding associates a configured Node with an Interface, Endpoint, Service, resource, Dependency, communication channel, data source, data destination, Credential, Policy, or other external participant required for operation.

The Node Binding identifies both participants, the relationship between them, and the conditions governing their interaction. This permits the DIDO-TE to determine whether the intended Node communicates with the intended counterpart through an approved mechanism.

An absent, incorrect, incompatible, ambiguous, or unauthorized Node Binding may direct data or control to the wrong participant, prevent required interaction, or compromise Test Environment isolation.

Applies To

[[dido:99_annexes:annex-b-terms-and-definitions:t:test_environment|Test