C.3.3 Twin Node Requirements

Go to C.3 Functional Requirements

This section identifies the requirements governing Twin Nodes used to represent, reproduce, observe, compare, or interact with the behavior of corresponding Nodes within distributed verification and testing.

Twin Node requirements address the controlled relationship between a Twin Node and the Node, system, service, or behavior it represents, including identity, configuration, state, synchronization, observation, substitution, comparison, and traceability.

The requirements in this section derive from the applicable source documents identified in Annex B. Some requirements derive directly from those sources. Others normalize or decompose source concepts into individually verifiable architectural obligations.

A Twin Node requirement may be represented by an individual leaf requirement or by a non-leaf requirement group containing subordinate independently verifiable obligations.

Requirements

Contents

Notes for Editors

Twin Node requirements use the TWIN requirement prefix.

The explicit links under Contents remain while the Twin Node requirement pages are being created and reviewed. After all planned requirement pages exist, the explicit links may be removed because the indexmenu automatically discovers them.

Preserve stable requirement identifiers when moving or reorganizing Twin Node requirement pages.

Apply the requirement identification, decomposition, source and derivation, normative-language, quality, status, and page-structure rules defined by Annex C.

Do not allocate Twin Node requirements directly to a particular product or realization within the requirement Statement. Maintain realization relationships through Traceability.

© 2026 Dido Solutions, Inc. and Jackrabbit Consulting, Inc.