ENV-002b — Instantiate Included Test Objects

Go to ENV-002 — Configure Test Environment

Statement

The DIDO-TE SHALL instantiate each Test Object included in a Test Environment before Test Execution.

Derived From

, source requirement identifier and obligation to be assigned[DTE6] Structured Information Processing Reference Architecture (SIP-RA)[DTE7] Federated Data Interpretation Systems Reference Architecture (FDIS-RA)

Rationale

Instantiating each included Test Object establishes the actual object subjected to evaluation during Test Execution.

The instantiated Test Object provides the operating instance against which the applicable Test Definition, inputs, procedures, and expected outcomes apply.

Establishing correspondence between the defined Test Object and its instantiated state supports Traceability, repeatable Test Execution, and interpretation of the resulting Test Results.

Applies To

Verification

Verification confirms that:

The DIDO-TE instantiates every Test Object included in the Test Environment.Each instantiated Test Object corresponds to a Test Object identified by the controlled Test Environment information.Each instantiated Test Object has the specified version, Baseline, and Configuration.Each instantiated Test Object enters its required initial state before Test Execution.The DIDO-TE maintains Traceability between each defined Test Object and its instantiated state.A missing, incorrect, or untraceable Test Object instance constitutes nonconformance with this requirement.Verification includes:

Inspection of the Test Objects identified for the Test EnvironmentInspection of each instantiated Test ObjectComparison of each instantiated Test Object with its controlled definitionInspection of the version, Baseline, Configuration, and initial state of each instantiated Test ObjectInspection of Traceability records connecting each defined Test Object to its instantiated stateA negative assessment using a missing, incorrect, or untraceable Test Object instanceConfirmation that the negative assessment produces a nonconformance result

Referenced By

Related Architecture Sections

Add links to the architecture sections governing Test Objects, Test Environment instantiation, and Test Object lifecycle.

Delivery Phase

Assign the applicable delivery phase.

Requirement Status

Draft

Statement Reference

Use the following syntax to reference this requirement’s Statement section from another DokuWiki page:

{{section>dido:03-dido-te:99-annexes:annex-c-requirements:02-test-environment-requirements:env-002-configure-test-environment:env-002b-instantiate-included-test-objects#Statement&noheader&nofooter&noeditbtn}}

© 2026 Dido Solutions, Inc. and Jackrabbit Consulting, Inc.