ENV-002d — Provision Required Test Resources

Go to ENV-002 — Configure Test Environment

Statement

The DIDO-TE SHALL provision each Test Resource required by a Test Environment before Test Execution.

Derived From

, source requirement identifier and obligation to be assigned[DTE6] Structured Information Processing Reference Architecture (SIP-RA)[DTE7] Federated Data Interpretation Systems Reference Architecture (FDIS-RA)

Rationale

Provisioning each required Test Resource establishes the supporting capabilities, services, data, equipment, software, credentials, or facilities required by a Test Environment.

Provisioning the required Test Resources before Test Execution prevents unavailable, incorrect, or uncontrolled resources from affecting execution or the resulting Test Results.

Establishing correspondence between each specified Test Resource and its provisioned instance supports Traceability, Reproducibility, and assessment of resource-related differences between Test Executions.

Applies To

Verification

Verification confirms that:

The DIDO-TE provisions every Test Resource required by the Test Environment.Each provisioned Test Resource corresponds to a Test Resource identified by the controlled Test Environment information.Each provisioned Test Resource has the specified version, Baseline, Configuration, capacity, and availability.Each provisioned Test Resource resides on or remains accessible from the applicable Deployment Target.Each provisioned Test Resource enters its required initial state before Test Execution.The DIDO-TE maintains Traceability between each specified Test Resource and its provisioned instance.A missing, incorrect, unavailable, or untraceable Test Resource constitutes nonconformance with this requirement.Verification includes:

Inspection of the Test Resources specified for the Test EnvironmentInspection of each provisioned Test ResourceComparison of each provisioned Test Resource with its controlled definitionInspection of the version, Baseline, Configuration, capacity, availability, and initial state of each provisioned Test ResourceInspection of Traceability records connecting each specified Test Resource to its provisioned instanceA negative assessment using a missing, incorrect, unavailable, or untraceable Test ResourceConfirmation that the negative assessment produces a nonconformance result

Referenced By

Related Architecture Sections

Add links to the architecture sections governing Test