P2-REQ-16-4-003

Return to Requirements

Statement

A Logical Communication Endpoint SHALL identify a platform-independent point of information exchange among Logical Nodes.

Source

Part 2, Section 16.4: Logical Communication Requirements.

Rationale

Logical Communication Endpoints provide the architectural abstraction through which Logical Nodes exchange information. Treating endpoints as platform-independent concepts preserves architectural meaning while allowing different implementation technologies to realise the same logical communication relationships.

Applies To

This requirement applies to Logical Communication Endpoints throughout the Logical Architecture / PIM.

It applies specifically to:

Logical Communication Endpoints;Logical Nodes;Logical interactions; andCommunication modelling.

Verification

Verification SHALL confirm that every Logical Communication Endpoint identifies a platform-independent point of information exchange among Logical Nodes.

Verification activities should include review checks confirming that:

Logical Communication Endpoints are explicitly identified;Logical Communication Endpoints connect Logical Nodes;endpoint definitions remain independent of implementation technologies; andLogical Communication Endpoints support logical interaction modelling.

Traceability

This requirement supports traceability between Logical Communication Endpoints, participating Logical Nodes, and Logical Interaction Patterns.

Related requirement identifiers:

Related source section:

Status

Draft

© 2026 Dido Solutions, Inc. and Jackrabbit Consulting, Inc.