10.6 Issue Control Command

Go To Top

The Issue Control Command pattern allows a Logical Node to request or direct operational action by another Logical Node or Logical Node Role.

A command-producing Logical Node issues a Logical Command through a Logical Communication Endpoint. The command identifies the intended action, target Logical Node or role, command identifier, timestamp, expected acknowledgement, authorizing condition, and Traceability expectations.

The interaction belongs primarily to the Logical Control Plane. It also supports the Logical Audit and Provenance Plane by recording command issuance for review or Evidence.

Table 10-5: Issue Control Command logical interaction pattern

Element	Logical treatment
Primary Runtime Plane	Logical Control Plane
Producing Logical Node Role	Command Producer, Control Node, Coordinator, or Operator-facing Node
Consuming Logical Node Role	Command Consumer, Managed Node, Worker Node, or Controlled Node
Primary information	Logical Command
Supporting information	Command identifier, target Node or role, intended action, timestamp, authorizing condition
Traceability expectation	Command traces to producing Logical Node, target Node or role, command definition, and authorizing condition.
Evidence expectation	Command record supports review of operational control and later reconstruction.

© 2026 Dido Solutions, Inc. and Jackrabbit Consulting, Inc.