14.6 Configuration Directory Model

Go To Phase 0 Repository and Build Artifact Model

The configuration directory contains implementation configuration artifacts for Phase 0.

Configuration artifacts may include DDS configuration, QoS profile files, topic mapping configuration, node identity configuration, runtime parameter files, logging configuration, and other implementation settings selected for the Phase 0 baseline.

Configuration files must identify their purpose, affected implementation participants, affected DDS Topics or QoS profiles, related Runtime Plane where applicable, and relationship to the implementation baseline.

Configuration artifacts support implementation behavior. They do not redefine FX logical Nodes, FX logical Communication Endpoints, FX logical information structures, Runtime Planes, or interaction patterns.

© 2026 Dido Solutions, Inc. and Jackrabbit Consulting, Inc.